Mercury API
CmdHibikiWriteMultipleWords Method (timeout, accessPassword, bank, wordOffset, data)
Namespaces ► ThingMagic ► SerialReader ► CmdHibikiWriteMultipleWords(UInt16, UInt32, Gen2..::.Bank, UInt32, ICollection<(Of <(Byte>)>))
Send the Hitachi Hibiki Write Multiple Words Lock command.
Declaration Syntax

C# | Visual Basic | Visual C++

    [ObsoleteAttribute]
    public void CmdHibikiWriteMultipleWords(
    	ushort timeout,
    	uint accessPassword,
    	Gen2..::.Bank bank,
    	uint wordOffset,
    	ICollection<byte> data
    )

    <ObsoleteAttribute> _
    Public Sub CmdHibikiWriteMultipleWords ( _
    	timeout As UShort, _
    	accessPassword As UInteger, _
    	bank As Gen2..::.Bank, _
    	wordOffset As UInteger, _
    	data As ICollection(Of Byte) _
    )

    [ObsoleteAttribute]
    public:
    void CmdHibikiWriteMultipleWords(
    	unsigned short timeout,
    	unsigned int accessPassword,
    	Gen2..::.Bank bank,
    	unsigned int wordOffset,
    	ICollection<unsigned char>^ data
    )

Parameters

timeout (UInt16)
  the timeout of the operation, in milliseconds. Valid range is 0-65535.

accessPassword (UInt32)
  the access password to use to write to the tag

bank (Gen2..::.Bank)
  the Gen2 memory bank to write to

wordOffset (UInt32)
  the word address to start writing at

data (ICollection <(Of <( Byte >)>))
  the data to write - must be an even number of bytes

Assembly: MercuryAPI (Module: MercuryAPI) Version: 1.29.4.34 (1.29.4.34)