Mercury API
ThingMagic Namespace
Namespaces ► ThingMagic
Namespace contains ThingMagic Specific Implementations
Declaration Syntax

C# | Visual Basic | Visual C++

    namespace ThingMagic

    Namespace ThingMagic

    namespace ThingMagic

Types

All Types | Classes | Interfaces | Enumerations | Delegates

Icon | Type | Description
--- | --- | ---
| Gen2..::.IDS..::.SL900A..::.AccessFifo | SL900A Access FIFO Tagop
| Gen2..::.IDS..::.SL900A..::.AccessFifoRead | AccessFifo "Read" tagop
| Gen2..::.IDS..::.SL900A..::.AccessFifoStatus | AccessFifo "Read Status" tagop
| Gen2..::.IDS..::.SL900A..::.AccessFifoWrite | AccessFifo "Write" tagop
| Gen2..::.Denatran..::.IAV..::.ActivateSecureMode | PA Protocol - Activate secure mode
| Gen2..::.Denatran..::.IAV..::.ActivateSiniavMode | Activate Siniav mode - G0 Protocol
| Gen2..::.NXP..::.AES | AES class
| Gen2..::.Alien | Alien vendor type
| SerialReader..::.AntennaPort | Object representing state of reader's antennas
| SerialReader..::.AntennaSelection | Options for Read Tag Multiple
| AntennaStatusReport | AntennaStatusReport
| Gen2..::.IDS..::.SL900A..::.ApplicationData | Logging memory configuration
| Ata | ATA tag-specific constructs
| Gen2..::.Authenticate | Authenticate
| Gen2..::.NXP..::.AES..::.Authenticate | Authenticate
| Gen2..::.Denatran..::.IAV..::.AuthenticateOBU | PA Protocol - Authenticate OBU
| Gen2..::.Bank | Gen2 memory bank identifiers
| Gen2..::.BAPParameters | BAP timing control parameters
| Gen2..::.IDS..::.SL900A..::.BatteryLevelReading | IDS SL900A Get Battery Level reply value
| Gen2..::.IDS..::.SL900A..::.BatteryType | Request the battery type re-check
| Gen2..::.BlockErase | BlockErase
| Gen2..::.BlockPermaLock | BlockPermalock
| Gen2..::.Alien..::.Higgs3..::.BlockReadLock | Higgs3BlockReadLock
| Gen2..::.BlockWrite | BlockWrite
| ByteConv | Convert numeric fields within M5e messages
| ByteFormat | Convert byte arrays to and from human-readable strings
| ByteIO | Read numeric fields from binary streams
| Gen2..::.NxpGen2TagOp..::.Calibrate | NxpCalibrate
| Gen2..::.NXP..::.G2X..::.Calibrate | NxpCalibrate
| Gen2..::.NXP..::.G2I..::.Calibrate | NxpCalibrate
| Gen2..::.IDS..::.SL900A..::.CalibrationData | Calibration parameters
| Gen2..::.IDS..::.SL900A..::.CalSfe | Combination Calibration Data / SFE Parameters object (as received from Get Calibration Data command)
| Gen2..::.NXP..::.G2I..::.ChangeConfig | NXP Config Change
| Gen2..::.NXP..::.UCODE7..::.ChangeConfig | NXP Config Change
| Gen2..::.NxpGen2TagOp..::.ChangeEas | NxpChangeEas
| Gen2..::.NXP..::.G2X..::.ChangeEas | ChangeEas
| Gen2..::.NXP..::.G2I..::.ChangeEas | ChangeEas
| SerialReader..::.CmdOpcode | command opcode for multi-protocol search
| CollUtil | ICollection conversion routines
| SerialReader..::.Configuration | Reader Parameter Identifiers
| Gen2..::.NXP..::.G2I..::.ConfigWord | ConfigWord
| Gen2..::.NXP..::.UCODE7..::.ConfigWord | ConfigWord
| Reader..::.DebugLog | Debug logging interface for Reader and subclasses
| Gen2..::.IDS..::.SL900A..::.Delay | Delay Time structure for Initialize command
| Gen2..::.IDS..::.SL900A..::.DelayMode | Data log memory-full behavior
| Iso180006b..::.Delimiter | Iso180006b Delimiter Value
| Gen2..::.Denatran | IAVDenatran secure tag operations.
| Gen2..::.DenatranIAVWriteCredential | Denatran IAV write credential
| Gen2..::.DenatranIAVWriteSecCredential | Denatran IAV writesec credential
| Reader..::.DiskLog | Send debug log to disk
| Disposable | abstraft class which implements the Dispose Pattern
| Gen2..::.DivideRatio | Divide Ratio values
| Reader..::.DummyDebugLog | Dummy DiskLog class for disabling logging without removing debug statements
| Gen2..::.DynamicQ | Gen2 Dynamic Q subclass.
| Gen2..::.NxpGen2TagOp..::.EasAlarm | NxpChangeEas
| Gen2..::.NXP..::.G2X..::.EasAlarm | EasAlarm
| Gen2..::.NXP..::.G2I..::.EasAlarm | EasAlarm
| Gen2..::.IDS..::.SL900A..::.EndLog | SL900A End Log tagop
| Gen2..::.Untraceable..::.EPC | Gen2v2 untraceably hides part of EPC memory or not
| Gen2..::.Alien..::.Higgs3..::.FastLoadImage | Higgs3FastLoadImage
| FAULT_AFE_NOT_ON_Exception | Reader not fully initialized and hasn't yet turned on its radio. Have you set region?
| FAULT_AHAL_ANTENNA_NOT_CONNECTED_Exception | Antenna not detected during pre-transmit safety test
| FAULT_AHAL_CHANNEL_OCCUPIED_Exception | Internal reader error. Contact support.
| FAULT_AHAL_HIGH_RETURN_LOSS_Exception | Excess power detected at transmitter port, usually due to antenna tuning mismatch.
| FAULT_AHAL_INVALID_FREQ_Exception | Internal reader error. Contact support.
| FAULT_AHAL_TEMPERATURE_EXCEED_LIMITS_Exception | Reader temperature outside safe range
| FAULT_AHAL_TRANSMITTER_ON_Exception | Internal reader error. Contact support.
| FAULT_BL_INVALID_APP_END_ADDR_Exception | Firmware corruprt: Internal address marker is invalid.
| FAULT_BL_INVALID_IMAGE_CRC_Exception | Firmware is corrupt: Checksum doesn't match content.
| FAULT_DATA_TOO_LARGE_Exception | Read Tag Data was asked for more data than it supports.
| FAULT_FLASH_BAD_ERASE_PASSWORD_Exception | Internal reader error. Contact support.
| FAULT_FLASH_BAD_WRITE_PASSWORD_Exception | Internal reader error. Contact support.
| FAULT_FLASH_ILLEGAL_SECTOR_Exception | Internal reader error. Contact support.
| FAULT_FLASH_UNDEFINED_ERROR_Exception | Internal reader error. Contact support.
| FAULT_FLASH_VERIFY_FAILED_Exception | Internal reader error. Contact support.
| FAULT_FLASH_WRITE_TO_ILLEGAL_SECTOR_Exception | Internal reader error. Contact support.
| FAULT_FLASH_WRITE_TO_NON_ERASED_AREA_Exception | Internal reader error. Contact support.
| FAULT_GEN2_PROTOCOL_INSUFFICIENT_POWER_Exception | Internal reader error. Contact support.
| FAULT_GEN2_PROTOCOL_MEMORY_LOCKED_Exception | Internal reader error. Contact support.
| FAULT_GEN2_PROTOCOL_MEMORY_OVERRUN_BAD_PC_Exception | Internal reader error. Contact support.
| FAULT_GEN2_PROTOCOL_NON_SPECIFIC_ERROR_Exception | Internal reader error. Contact support.
| FAULT_GEN2_PROTOCOL_OTHER_ERROR_Exception | Internal reader error. Contact support.
| FAULT_GEN2_PROTOCOL_UNKNOWN_ERROR_Exception | Internal reader error. Contact support.
| FAULT_GEN2_PROTOCOL_V2_AUTHEN_FAILED_Exception | Gen2v2 tag authentication failed.
| FAULT_GEN2_PROTOCOL_V2_UNTRACE_FAILED_Exception | Gen2v2 Untraceable operation failed.
| FAULT_GENERAL_TAG_ERROR_Exception | Unknown error during RFID operation.
| FAULT_INVALID_BAUD_RATE_Exception | Requested serial speed is not supported.
| FAULT_INVALID_LICENSE_KEY_Exception | Command opcode not recognized.
| FAULT_INVALID_OPCODE_Exception | Command opcode not recognized.
| FAULT_INVALID_PROTOCOL_SPECIFIED_Exception | Requested RFID protocol is not recognized.
| FAULT_INVALID_REGION_Exception | Region is not supported.
| FAULT_MSG_INVALID_FREQ_RECEIVED_Exception | Requested frequency is outside the allowed range.
| FAULT_MSG_INVALID_PARAMETER_VALUE_Exception | Parameter value is outside the allowed range.
| FAULT_MSG_POWER_TOO_HIGH_Exception | Requested power setting is above the allowed maximum.
| FAULT_MSG_POWER_TOO_LOW_Exception | Requested power setting is below the allowed minimum.
| FAULT_MSG_WRONG_NUMBER_OF_DATA_Exception | Invalid number of arguments
| FAULT_NO_PROTOCOL_DEFINED_Exception | RFID protocol has not been configured.
| FAULT_NO_TAGS_FOUND_Exception | Reader was asked to find tags, but none were detected.
| FAULT_NOT_IMPLEMENTED_FOR_THIS_PROTOCOL_Exception | Command is not supported in the current RFID protocol.
| FAULT_PROTOCOL_BIT_DECODING_FAILED_Exception | Internal reader error. Contact support.
| FAULT_PROTOCOL_INVALID_ADDRESS_Exception | Requested data address is outside the valid range.
| FAULT_PROTOCOL_INVALID_EPC_Exception | Invalid epc value was specified for an operation.
| FAULT_PROTOCOL_INVALID_KILL_PASSWORD_Exception | Incorrect password was provided to Kill Tag.
| FAULT_PROTOCOL_INVALID_NUM_DATA_Exception | Invalid data was specified for an operation
| FAULT_PROTOCOL_INVALID_WRITE_DATA_Exception | Data does not conform to protocol standards. For example, EPC0 and EPC1 require EPC header bits to match the length of the EPC, as defined in the EPCGlobal Tag Data Standard.
| FAULT_PROTOCOL_KILL_FAILED_Exception | Kill failed for unknown reason.
| FAULT_PROTOCOL_NO_DATA_READ_Exception | Tag data was requested, but could not be read.
| FAULT_PROTOCOL_WRITE_FAILED_Exception | Write to tag failed.
| FAULT_SYSTEM_UNKNOWN_ERROR_Exception | Internal reader error. Contact support.
| FAULT_TAG_ID_BUFFER_AUTH_REQUEST_Exception | Asked for tags than a single transaction can handle.
| FAULT_TAG_ID_BUFFER_FULL_Exception | Too many tags are in buffer. Remove some with Get Tag ID Buffer or Clear Tag ID Buffer.
| FAULT_TAG_ID_BUFFER_NOT_ENOUGH_TAGS_AVAILABLE_Exception | Asked for more tags than were available in the buffer.
| FAULT_TAG_ID_BUFFER_NUM_TAG_TOO_LARGE_Exception | Asked for tags than a single transaction can handle.
| FAULT_TAG_ID_BUFFER_REPEATED_TAG_ID_Exception | Internal error -- reader is trying to insert a duplicate tag record. Contact support.
| FAULT_TM_ASSERT_FAILED_Exception | Internal reader error. Contact support.
| FAULT_UNIMPLEMENTED_FEATURE_Exception | Command not supported.
| FAULT_UNIMPLEMENTED_OPCODE_Exception | Command opcode recognized, but is not supported.
| FAULT_WRITE_PASSED_LOCK_FAILED_Exception | For write-then-lock commands, tag was successfully written, but lock failed.
| FeatureNotSupportedException | Non-fatal exception used to signal that a feature is not supported, therefore any dependent features should also be disabled.
| Gen2..::.IDS..::.SL900A..::.FifoSource | Source of FIFO data
| Gen2..::.IDS..::.SL900A..::.FifoStatus | FIFO Status return value
| FirmwareLoadOptions | Firmware load options
| FixedReaderFirmwareLoadOptions | Firmware load options
| SerialReader..::.FrequencyHopTableOption | Frequency hoptable options
| FrequencyStatusReport | FrequencyStatusReport
| Gen2..::.Alien..::.Higgs2..::.FullLoadImage | Higgs2FullLoadImage
| Gen2..::.Denatran..::.IAV..::.G0PAOBUAuth | G0PAOBUAuth - G0-PA Protocol
| Gen2..::.NXP..::.G2I | G2I class
| Gen2..::.NXP..::.G2X | G2X class
| Gen2 | Gen2 protocol-specific constructs
| Gen2..::.Gen2_SiliconType | Enums for silicon types
| SerialReader..::.Gen2Configuration | Option key value for serial Set Protocol Configuration command
| Gen2..::.Gen2CustomTagOp | Gen2CustomTagOp
| Gen2..::.IDS..::.SL900A..::.GetBatteryLevel | SL900A Get Battery Level Tagop
| Gen2..::.IDS..::.SL900A..::.GetCalibrationData | SL900A Get Calibration Data tagop
| Gen2..::.IDS..::.SL900A..::.GetLogState | SL900A Get Log State tagop
| Gen2..::.IDS..::.SL900A..::.GetMeasurementSetup | SL900A Get Measurement Setup Tagop
| Gen2..::.IDS..::.SL900A..::.GetSensorValue | SL900A Get Sensor Value Tagop
| Gen2..::.Denatran..::.IAV..::.GetTokenId | G0 Protocol - Get TokedId.
| GpioPin | Class representing GPIO pin number and state
| GpiPinTrigger | This class represents gpiPinTrigger.
| SerialReader..::.HibikiSystemInformation | Hibiki System Information.
| Gen2..::.Alien..::.Higgs2 | Higgs2
| Gen2..::.Alien..::.Higgs3 | Higgs3
| Gen2..::.Denatran..::.IAV | Protocol
| Gen2..::.IDS | IDS Microchip Custom Gen2 Tag Operations
| Gen2..::.Impinj | Impinj microchip custom Gen2 Tag operations
| Gen2..::.IDS..::.SL900A..::.Initialize | SL900A Initialize Tagop
| IntUtil | Integer conversion routines
| Ipx256 | ISO tag-specific constructs for Ipx256
| Ipx64 | Iso tag-specific constructs
| Iso180006b | Iso tag-specific constructs
| SerialReader..::.Iso180006bConfiguration | Option key values for serial Set Protocol Configuration command
| Iso180006bUcode | Iso180006bUcode tag-specific constructs
| Gen2..::.NXP..::.AES..::.KeyId | Authentication KeyId
| Gen2..::.Kill | Embedded Tag Operation: Kill
| Gen2..::.IDS..::.SL900A..::.Level | SL900A password access level values
| Reader..::.LicenseOperation | Class for License key operation
| Reader..::.LicenseOption | Operation Options for CmdSetProtocolLicenseKey
| Gen2..::.IDS..::.SL900A..::.LimitCounter | Sensor limit excursion counters
| Gen2..::.LinkFrequency | Gen2 LinkFrequency
| Iso180006b..::.LinkFrequency | enum to define link frequency options
| LlrpFirmwareLoadOptions | Fixed reader firmware load options
| LlrpReader | The RqlReader class is an implementation of a Reader object that communicates with a ThingMagic fixed RFID reader via the Low level reader protocol. Instances of the Llrp class are created with the Reader.create()method with a "llrp" URI or a generic "tmr" URI that references a network device.
| Gen2..::.Alien..::.Higgs3..::.LoadImage | Higgs3FastLoadImage
| Gen2..::.Lock | Embedded Tag Operation: Lock
| Gen2..::.LockAction | Gen2 lock action specifier
| Iso180006b..::.LockAction | Iso180006B lockAction
| Iso180006b..::.LockTag | Perform a lock or unlock operation on a tag. The first tag seen is operated on - the singulation parameter may be used to control this. Note that a tag without an access password set may not accept a lock operation or remain locked.
| Gen2..::.IDS..::.SL900A..::.LoggingForm | Data log format selection
| Reader..::.LogHandler | Target pattern for debug log messages
| Gen2..::.IDS..::.SL900A..::.LogLimit | Log limit parameters
| Gen2..::.IDS..::.SL900A..::.LogModeData | SL900A Log Mode Data
| Gen2..::.IDS..::.SL900A..::.LogState | Get Log State reply
| M5eException | M5e-related exception
| M5eStatusException | Error status code returned from M5e
| Gen2..::.Impinj..::.Monza6..::.MarginRead | Monza6 MarginRead
| Gen2..::.IDS..::.SL900A..::.MeasurementSetupData | Measurement Setup Data object (as received from Get Measurement Setup Data command)
| Iso180006b..::.ModulationDepth | Iso180006b Modulation Depth Value
| Gen2..::.Impinj..::.Monza4 | Monza4 tag operations
| Gen2..::.Impinj..::.Monza6 | Monza6 tag operations
| Gen2..::.Impinj..::.Monza6..::.Monza6SubCmd | Enums for Monza6 subcommands
| MultiFilter | This represents an ordered sequence of filter operations.
| MultiReadPlan | ReadPlan containing a list of read plans to be executed sequentially with time divided according to relative weights.
| Gen2..::.NXP | NXP vendor type
| Gen2..::.NxpGen2TagOp | NXP Gen2 Tag Operation
| Gen2..::.Denatran..::.IAV..::.OBUAuthFullPass | G0 Protocol - Unilateral OBU Authentication with full read of page 1 of USER memory, full pass.
| Gen2..::.Denatran..::.IAV..::.OBUAuthFullPass1 | G0 Protocol - Unilateral OBU Authentication with full read of page 1 of USER memory, pass 1.
| Gen2..::.Denatran..::.IAV..::.OBUAuthFullPass2 | G0 Protocol - Unilateral OBU Authentication with full read of page 1 of USER memory, pass 2.
| Gen2..::.Denatran..::.IAV..::.OBUAuthID | G0 Protocol - Unilateral OBU authentication and identification.
| Gen2..::.Denatran..::.IAV..::.OBUReadFromMemMap | G0 Protocol - OBUReadFromMemMap
| Gen2..::.Denatran..::.IAV..::.OBUWriteToMemMap | G0 Protocol - OBUWriteToMemMap
| Gen2..::.Alien..::.Higgs2..::.PartialLoadImage | Higgs2PartialLoadImage
| Gen2..::.Password | Stores a 32-bit Gen2 password for use as an access or kill password.
| Reader..::.Stat..::.PerAntennaValues | Per Antenna stats
| Reader..::.PowerMode | enum to define different power modes.
| Gen2..::.NXP..::.AES..::.Profile | Memory profile for the addition of custom data
| SerialReader..::.ProtocolBitMask | protocol bitmask
| SerialReader..::.ProtocolConfiguration | Interface to define Protocol Configurations.
| Gen2..::.ProtocolExtension | Gen2 Protocol Extesnion Value
| ProtocolTagReadData | An abstract class which can be extended for specific protocol. Currently Gen2TagReadData for Gen2 protocol
| Gen2..::.Q | Abstract Gen2 Q class.
| Gen2..::.Impinj..::.Monza4..::.QTControlByte | Monza4 QT Control Byte
| Gen2..::.Impinj..::.Monza4..::.QTPayload | Monza QT Payload
| Gen2..::.Impinj..::.Monza4..::.QTReadWrite | Monza4 QTReadWrite
| Gen2..::.Untraceable..::.Range | specifies Gen2v2 Tag’s operating range
| ReadAuthenticationEventArgs | Read Authentication Event Args class
| Gen2..::.ReadBuffer | ReadBuffer
| Gen2..::.NXP..::.AES..::.ReadBuffer | ReadBuffer
| Gen2..::.ReadData | Embedded Tag Operation: Read Data
| Iso180006b..::.ReadData | Read data from the memory bank of a tag.
| Reader | Abstract base class for ThingMagic RFID reader devices.
| ReaderCodeException | Thrown when an error code is recieved from a reader device
| ReaderCommException | Reader communication exception
| ReaderException | Reader-related exceptions
| ReaderExceptionEventArgs | Reader Exception Event Args class
| Reader..::.ReaderFactory | Creates a Reader factory method.
| ReaderFatalException | Thrown when there is an error that cannot be recovered from
| ReaderParseException | Thrown when there is an error parsing a message returned from the device
| SerialReader..::.ReaderStatistics | Reader Statistics class.
| SerialReader..::.ReaderStatisticsFlag | Reader Statistics Flag enum
| ReaderStatsReport | ReaderStatsReport
| Reader..::.ReaderStatusFlag | Reader Status Flag enum
| Reader..::.ReadExceptionPublisher | Publishes ReadException
| ReadPlan | Tag read (search) constraints
| Gen2..::.Denatran..::.IAV..::.ReadSec | IP63 Protocol - ReadSec
| Reader..::.Region | RFID regulatory regions
| SerialReader..::.RegionConfiguration | Region-specific parameters that are supported on the device.
| Gen2..::.NxpGen2TagOp..::.ResetReadProtect | NxpSetReadProtect
| Gen2..::.NXP..::.G2X..::.ResetReadProtect | ResetReadProtect
| Gen2..::.NXP..::.G2I..::.ResetReadProtect | ResetReadProtect
| RqlFirmwareLoadOptions | Fixed reader firmware load options
| RqlReader | The RqlReader class is an implementation of a Reader object that communicates with a ThingMagic fixed RFID reader via the RQL network protocol. Instances of the RQL class are created with the Reader.create()method with a "rql" URI or a generic "tmr" URI that references a network device.
| Gen2..::.SecurePasswordLookup | Secure Read Data : SecurePasswordLookup
| Gen2..::.SecureReadData | Embedded Tag Operation: Secure Read Data
| Gen2..::.Denatran..::.IAV..::.SecureTagOpType | Enum IAVDenatran secure tag operation
| Gen2..::.SecureTagType | Enum SecureTagType Default, Alien Higgs 3 and Monza 4 QT
| Gen2..::.Select | Representation of a Gen2 Select operation
| Iso180006b..::.Select | Representation of a ISO Select Operation.
| Iso180006b..::.SelectOp | enum to define select options
| Gen2..::.IDS..::.SL900A..::.Sensor | SL900A sensor type values
| Gen2..::.IDS..::.SL900A..::.SensorReading | IDS SL900A Get Sensor Value reply value
| SerialFirmwareLoadOptions | Serial reader firmware load options

SerialReader

The SerialReader class is an implementation of a Reader object that communicates with a ThingMagic embedded RFID module via the embedded module serial protocol. In addition to the Reader interface, direct access to the commands of the embedded module serial protocol is supported. Instances of the SerialReader class are created with the {@link #com.thingmagic.Reader.create} method with a "eapi" URI or a generic "tmr" URI that references a local serial port.

| SerialReader..::.SerialTagProtocol | Tag Protocol identifiers, as used in Get and Set Current Tag Protocol
| SerialTransport | Serial transport
| SerialTransportNative | Serial transport native framework calls
| SerialTransportTCP | Serial transport TCP framework calls
| Gen2..::.Session | Gen2 Session settings.
| Gen2..::.IDS..::.SL900A..::.SetCalibrationData | SL900A Set Calibration Data tagop
| Gen2..::.IDS..::.SL900A..::.SetLogLimit | SL900A Set log limit tagop
| Gen2..::.IDS..::.SL900A..::.SetLogMode | SL900A Set Log Mode Tagop
| Gen2..::.IDS..::.SL900A..::.SetPassword | SL900A Set Password Tagop
| Gen2..::.NxpGen2TagOp..::.SetReadProtect | NxpSetReadProtect
| Gen2..::.NXP..::.G2X..::.SetReadProtect | SetReadProtect
| Gen2..::.NXP..::.G2I..::.SetReadProtect | SetReadProtect
| Gen2..::.IDS..::.SL900A..::.SetSfeParameters | SL900A Set SFE Parameters tagop
| Gen2..::.IDS..::.SL900A..::.SetShelfLife | SL900A Get Battery Level Tagop
| Reader..::.Setting | Parameter object
| Reader..::.SettingFilter | Parameter setting filter. Modifies parameter value on the way in or out of the Setting object.
| Gen2..::.IDS..::.SL900A..::.SfeParameters | Sensor Front End Parameters
| Gen2..::.IDS..::.SL900A..::.ShelfLifeBlock0 | ShelfLifeBlock0 values are intended as reference information purpose for the interrogator.
| Gen2..::.IDS..::.SL900A..::.ShelfLifeBlock1 | ShelfLifeBlock1 holds the information on the initial shelf life and initial temperature.
| SimpleReadPlan | ReadPlan consisting of list of antennas, tag protocol, filter and weight
| Gen2..::.IDS..::.SL900A | SL900A Sensor Logging Chip Protocol
| Gen2..::.IDS..::.SL900A..::.StartLog | SL900A Start Log tagop
| Reader..::.Stat | Reader stats object.
| Gen2..::.StaticQ | Gen2 Static Q subclass.
| Reader..::.Stat..::.StatsFlag | Reader Stats Flag Enum -
| StatsReportEventArgs | This object sends reader statics to StatusListener
| Gen2..::.IDS..::.SL900A..::.StatusFlags | Log Status Flags
| StatusReport | This object contains the information related to status reports sent by the module during continuous reading
| StatusReportEventArgs | This object sends reader statics to StatusListener
| StopOnTagCount | StopOnTagCount object which consists of N value i.e reader should stop after seeing N tags (or timeout)
| StopTrigger | Abstract base class
| StopTriggerReadPlan | StopTriggerReadPlan consisting of stopontagcount, list of antennas, tag protocol, filter and weight
| Gen2..::.IDS..::.SL900A..::.StorageRule | Logging memory-full behavior
| Gen2..::.IDS..::.SL900A..::.AccessFifo..::.SubcommandCode | AccessFifo subcommand values
| Gen2..::.IDS..::.SL900A..::.SystemStatus | Logging System Status
| TagAuthentication | The TagAuthentication class is a generic superclass for various authentication mechanisms for accessing and killing tags. See the per-protocol subclasses for details.
| Ata..::.TagData | ATA specific version of TagData.
| TagData | Data relating to the identity and content of a tag.
| Iso180006bUcode..::.TagData | ISO specific version of TagData.
| Gen2..::.TagData | Gen2-specific version of TagData
| Ipx64..::.TagData | iPx specific version of TagData.
| Ipx256..::.TagData | The data structure holding the data read from tag
| Iso180006b..::.TagData | ISO specific version of TagData.
| Gen2..::.TagEncoding | Gen2 Tag Encoding.
| TagFilter | Specifies a subset of tags; e.g., match on EPC, or select prefixes
| TagLockAction | Tag locking descriptor, to be implemented in protocol-specific subclasses, since each protocol can have radically different lock architectures.
| SerialReader..::.TagMetadataFlag | Enum to define the Tag Metadata.
| TagOp | Tag Operations for GEN2 Embbeded Command
| TagOpList | Tag Operations for GEN2 Embbeded Command
| TagProtocol | Tag protocol designator
| Gen2..::.TagReadData | Gen2-specific version of TagData
| TagReadData | Data representing the reading of an RFID tag
| TagReadDataEventArgs | Tag Read Data Event Args class
| TagsObservationTrigger | TagsObservationTrigger class
| Gen2..::.NXP..::.AES..::.Tam1Authentication | TAM1 authentication
| Gen2..::.NXP..::.AES..::.Tam2Authentication | TAM2 authentication
| Gen2..::.Target | Gen2 target settings. Includes standard A(0) and B(1), as well as ThingMagic reader values of A-then-B, and B-then-A
| Gen2..::.Tari | Gen2 Tari Value
| TemperatureStatusReport | TemperatureStatusReport
| Gen2..::.Untraceable..::.TID | Gen2v2 untraceably hides part of TID memory or not
| TransportListenerEventArgs | Listener gets notification of all messages going across the transport layer.
| Gen2..::.TrExt | TRext: Include extended preamble in Tag-to-Reader response?
| Trigger | This class represents for setting up trigger read to the module.
| Gen2..::.NXP..::.UCODE7 | UCODE7 class
| Gen2..::.NXP..::.UCODE7..::.UCODE7SubCmd | Enums for UCODE7 subcommands
| Gen2..::.Untraceable | Untraceable
| Gen2..::.NXP..::.AES..::.Untraceable | Untraceable
| SerialReader..::.UserConfigCategory | Congfig key for CmdSetUserProfile
| SerialReader..::.UserConfigOp | class for UserConfigOp
| SerialReader..::.UserConfigOperation | Operation Options for CmdSetUserProfile
| SerialReader..::.UserConfigType | The config values for CmdSetUserProfile
| Gen2..::.Untraceable..::.UserMemory | Gen2v2 untraceably hides part of UserMemory memory or not
| SerialReader..::.UserMode | enum to define different user modes.
| Reader..::.Stat..::.Values | Reader stats values
| SerialReader..::.VersionInfo | Parsed response to Get Version
| VersionNumber | This class represents a version number for a component of the module.
| Gen2..::.WriteData | Embedded Tag Operation: Write Data
| Iso180006b..::.WriteData | Write data to the memory bank of a tag.
| Gen2..::.WriteMode | The mode for write operation
| Gen2..::.Denatran..::.IAV..::.WriteSec | IP63 Protocol - WriteSec
| Gen2..::.WriteTag | Write a new ID to a tag.