# TMR_NXP_UCODE7_ConfigWord Union Reference

`#include <tmr_gen2.h>`

List of all members.

## Detailed Description

The argument to a ChangeConfig command for NXP UCODE 7 tags User can set the configWord directly using the 16 bit 'data' field. Otherwise, provides an option to individually set each flag. Instance of TMR_NXP_UCODE7_ConfigWord must be initialized before using either by declaring it as 'static' or by using the constructor routine TMR_init_NXP_UCODE7_ConfigWord() method.

## Member Data Documentation

unsigned TMR_NXP_UCODE7_ConfigWord::maxBackscatterStrength

Maximum backscatter strength (permanently stored in tag memory)

unsigned TMR_NXP_UCODE7_ConfigWord::parallelEncoding

Parallel Encoding flag

unsigned TMR_NXP_UCODE7_ConfigWord::psfAlarm

Least significant bit PSF alarm flag (Permanently stored in tag memory)

unsigned TMR_NXP_UCODE7_ConfigWord::RFU0

RFU 0

unsigned TMR_NXP_UCODE7_ConfigWord::RFU1

RFU 1

unsigned TMR_NXP_UCODE7_ConfigWord::RFU10

RFU 10

unsigned TMR_NXP_UCODE7_ConfigWord::RFU11

RFU 11

unsigned TMR_NXP_UCODE7_ConfigWord::RFU12

RFU 12

unsigned TMR_NXP_UCODE7_ConfigWord::RFU13

RFU 13

unsigned TMR_NXP_UCODE7_ConfigWord::RFU14

RFU 14

unsigned TMR_NXP_UCODE7_ConfigWord::RFU3

RFU 3

unsigned TMR_NXP_UCODE7_ConfigWord::RFU5

RFU 5

unsigned TMR_NXP_UCODE7_ConfigWord::RFU6

RFU 6

unsigned TMR_NXP_UCODE7_ConfigWord::RFU7

RFU 7

unsigned TMR_NXP_UCODE7_ConfigWord::RFU8

RFU 8

unsigned TMR_NXP_UCODE7_ConfigWord::tagPower

Tag Power flag

The documentation for this union was generated from the following file:

- tmr_gen2.h