Mercury API
POWERUPDELAY Property
Namespaces ► ThingMagic ► Gen2..::.BAPParameters ► POWERUPDELAY
Time delay until transmission of first command after interrogator power-up For BAP tags to perform effective duty cycling, this value should be several msecs. This value is specified in microseconds and defaults to 3000.
Declaration Syntax

C# | Visual Basic | Visual C++

    public int POWERUPDELAY { get; set; }

    Public Property POWERUPDELAY As Integer

    public:
    property int POWERUPDELAY {
    	int get ();
    	void set (int value);
    }

Assembly: MercuryAPI (Module: MercuryAPI) Version: 1.29.4.34 (1.29.4.34)