Mercury API
CmdIso180006bWriteTagData Method (timeout, address, data, filter)
Namespaces ► ThingMagic ► SerialReader ► CmdIso180006bWriteTagData(UInt16, Byte, array<Byte>[]()[], TagFilter)
Write data to an ISO180006B tag.
Declaration Syntax

C# | Visual Basic | Visual C++

    [ObsoleteAttribute]
    public void CmdIso180006bWriteTagData(
    	ushort timeout,
    	byte address,
    	byte[] data,
    	TagFilter filter
    )

    <ObsoleteAttribute> _
    Public Sub CmdIso180006bWriteTagData ( _
    	timeout As UShort, _
    	address As Byte, _
    	data As Byte(), _
    	filter As TagFilter _
    )

    [ObsoleteAttribute]
    public:
    void CmdIso180006bWriteTagData(
    	unsigned short timeout,
    	unsigned char address,
    	array<unsigned char>^ data,
    	TagFilter^ filter
    )

Parameters

timeout (UInt16)
  the duration in milliseconds to search for a tag to write to. Valid range is 0-65535

address (Byte)
  the byte address to start writing at

data (array< Byte >[]()[])
  the data to write - must be an even number of bytes

filter (TagFilter)
  a specification of the air protocol filtering to perform to find the tag

Assembly: MercuryAPI (Module: MercuryAPI) Version: 1.29.4.34 (1.29.4.34)