Mercury API
Gen2..::.IDS..::.SL900A..::.GetSensorValue Constructor (sensorType, passwordLevel, password)
Namespaces ► ThingMagic ► Gen2..::.IDS..::.SL900A..::.GetSensorValue ► Gen2..::.IDS..::.SL900A..::.GetSensorValue(Gen2..::.IDS..::.SL900A..::.Sensor, Gen2..::.IDS..::.SL900A..::.Level, UInt32)
Constructor to initialize the parameters of GetSensorValue
Declaration Syntax

C# | Visual Basic | Visual C++

    public GetSensorValue(
    	Gen2..::.IDS..::.SL900A..::.Sensor sensorType,
    	Gen2..::.IDS..::.SL900A..::.Level passwordLevel,
    	uint password
    )

    Public Sub New ( _
    	sensorType As Gen2..::.IDS..::.SL900A..::.Sensor, _
    	passwordLevel As Gen2..::.IDS..::.SL900A..::.Level, _
    	password As UInteger _
    )

    public:
    GetSensorValue(
    	Gen2..::.IDS..::.SL900A..::.Sensor sensorType,
    	Gen2..::.IDS..::.SL900A..::.Level passwordLevel,
    	unsigned int password
    )

Parameters

sensorType (Gen2..::.IDS..::.SL900A..::.Sensor)
  Which sensor to read

passwordLevel (Gen2..::.IDS..::.SL900A..::.Level)
  password level

password (UInt32)
  password

Assembly: MercuryAPI (Module: MercuryAPI) Version: 1.29.4.34 (1.29.4.34)