Mercury API
Gen2..::.IDS..::.SL900A..::.SfeParameters Class
Namespaces ► ThingMagic ► Gen2..::.IDS..::.SL900A ► Gen2..::.IDS..::.SL900A..::.SfeParameters
Sensor Front End Parameters
Declaration Syntax

C# | Visual Basic | Visual C++

    public class SfeParameters

    Public Class SfeParameters

    public ref class SfeParameters

Members

All Members | Constructors | Methods | Properties | Fields
Public Protected | Instance Static | Declared Inherited

Icon | Member | Description
--- | --- | ---
| Gen2..::.IDS..::.SL900A..::.SfeParameters(array<Byte>[]()[], Int32) | Create SFEParameters object from raw 2-byte reply
| AutorangeDisable | Use preset range
| Equals(Object) | Determines whether the specified Object is equal to the current Object. (Inherited from Object.)
| Ext1 | External sensor 1 type 00 -- linear resistive sensor 01 -- high impedance input (voltage follower), bridge 10 -- capacitive sensor with DC 11 -- capacitive or resistive sensor without DC
| Ext2 | External sensor 2 type 00 -- linear conductive sensor 01 -- high impedance input (voltage follower), bridge
| Finalize()()() | Allows an Object to attempt to free resources and perform other cleanup operations before the Object is reclaimed by garbage collection. (Inherited from Object.)
| GetHashCode()()() | Serves as a hash function for a particular type. (Inherited from Object.)
| GetType()()() | Gets the Type of the current instance. (Inherited from Object.)
| MemberwiseClone()()() | Creates a shallow copy of the current Object. (Inherited from Object.)
| Rang | External sensor 2 range
| Raw | Raw 16-bit SFE parameters value
| Seti | External sensor 1 range
| ToString()()() | Human-readable representation (Overrides Object.ToString()()().)
| VerifySensorID | Sensor used in limit check 00 - first selected sensor 01 -- second selected sensor 10 -- third selected sensor 11 -- fourth selected sensor

Inheritance Hierarchy

Object
| Gen2..::.IDS..::.SL900A..::.SfeParameters

Assembly: MercuryAPI (Module: MercuryAPI) Version: 1.29.4.34 (1.29.4.34)