Mercury API
CmdWriteTagEpc Method (timeout, EPC, Lock)
Namespaces ► ThingMagic ► SerialReader ► CmdWriteTagEpc(UInt16, array<Byte>[]()[], Boolean)
Write the EPC of a tag and update the PC bits. Behavior is unspecified if more than one tag can be found.
Declaration Syntax

C# | Visual Basic | Visual C++

    [ObsoleteAttribute]
    public void CmdWriteTagEpc(
    	ushort timeout,
    	byte[] EPC,
    	bool Lock
    )

    <ObsoleteAttribute> _
    Public Sub CmdWriteTagEpc ( _
    	timeout As UShort, _
    	EPC As Byte(), _
    	Lock As Boolean _
    )

    [ObsoleteAttribute]
    public:
    void CmdWriteTagEpc(
    	unsigned short timeout,
    	array<unsigned char>^ EPC,
    	bool Lock
    )

Parameters

timeout (UInt16)
  the duration in milliseconds to search for a tag to write. Valid range is 0-65535

EPC (array< Byte >[]()[])
  the EPC to write to the tag

Lock (Boolean)
  whether to lock the tag (does not apply to all protocols)

Assembly: MercuryAPI (Module: MercuryAPI) Version: 1.29.4.34 (1.29.4.34)