Mercury API
Gen2..::.IDS..::.SL900A Class
Namespaces ► ThingMagic ► Gen2..::.IDS ► Gen2..::.IDS..::.SL900A
SL900A Sensor Logging Chip Protocol
Declaration Syntax

C# | Visual Basic | Visual C++

    public class SL900A : Gen2..::.IDS

    Public Class SL900A _
    	Inherits Gen2..::.IDS

    public ref class SL900A : public Gen2..::.IDS

Members

All Members | Constructors | Methods | Fields
Public Protected | Instance Static | Declared Inherited

Icon | Member | Description
--- | --- | ---
| Gen2..::.IDS..::.SL900A(Byte) | Default constructor
| Gen2..::.IDS..::.SL900A(Byte, Gen2..::.IDS..::.SL900A..::.Level, UInt32) | Constructor to initialize commandcode, password and passwordlevel
| AccessPassword | Gen2 access password
| ChipType | Chip Type (Inherited from Gen2..::.Gen2CustomTagOp.)
| CommandCode | Custom Command Code
| Equals(Object) | Determines whether the specified Object is equal to the current Object. (Inherited from Object.)
| Finalize()()() | Allows an Object to attempt to free resources and perform other cleanup operations before the Object is reclaimed by garbage collection. (Inherited from Object.)
| GetHashCode()()() | Serves as a hash function for a particular type. (Inherited from Object.)
| GetType()()() | Gets the Type of the current instance. (Inherited from Object.)
| MemberwiseClone()()() | Creates a shallow copy of the current Object. (Inherited from Object.)
| Password | IDS SL900A Password
| PasswordLevel | Access level to which SL900A password applies
| ToString()()() | Returns a String that represents the current Object. (Inherited from Object.)

Inheritance Hierarchy

Object
| TagOp
|  | Gen2..::.Gen2CustomTagOp
|  |  | Gen2..::.IDS
|  |  |  | Gen2..::.IDS..::.SL900A
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.AccessFifo
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.EndLog
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.GetBatteryLevel
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.GetCalibrationData
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.GetLogState
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.GetMeasurementSetup
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.GetSensorValue
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.Initialize
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.SetCalibrationData
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.SetLogLimit
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.SetLogMode
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.SetPassword
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.SetSfeParameters
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.SetShelfLife
|  |  |  |  | Gen2..::.IDS..::.SL900A..::.StartLog

Assembly: MercuryAPI (Module: MercuryAPI) Version: 1.29.4.34 (1.29.4.34)