# TMR_NXP_ConfigWord Union Reference

`#include <tmr_gen2.h>`

List of all members.

## Detailed Description

The argument to a ChangeConfig command for NXP G2iL tags User can set the configWord directly using the 16 bit 'data' field. Otherwise, provides an option to individually set each flag. Instance of TMR_NXP_ConfigWord must be initialized before using either by declaring it as 'static' or by using the constructor routine TMR_init_NXP_ConfigWord() method.

## Member Data Documentation

unsigned TMR_NXP_ConfigWord::conditionalReadRangeReduction_onOff

Conditional Read Range Reduction on/off (permanently stored in tag memory)

unsigned TMR_NXP_ConfigWord::conditionalReadRangeReduction_openShort

Conditional Read Range Reduction open/short (permanently stored in tag memory)

unsigned TMR_NXP_ConfigWord::dataMode

Transparent mode data/raw (reset at power up)

unsigned TMR_NXP_ConfigWord::digitalOutput

Digital output (permanently stored in tag memory)

unsigned TMR_NXP_ConfigWord::externalSupply

External supply flag digital input (read only)

unsigned TMR_NXP_ConfigWord::invertDigitalOutput

Invert digital output (reset at power up)

unsigned TMR_NXP_ConfigWord::maxBackscatterStrength

Maximum backscatter strength (permanently stored in tag memory)

unsigned TMR_NXP_ConfigWord::privacyMode

Read range reduction on/off (permanently stored in tag memory)

unsigned TMR_NXP_ConfigWord::psfAlarm

Least significant bit PSF alarm flag (Permanently stored in tag memory)

unsigned TMR_NXP_ConfigWord::readProtectEPC

Read protect EPC bank (Permanently stored in tag memory)

unsigned TMR_NXP_ConfigWord::readProtectTID

Read protect TID bank (permanently stored in tag memory)

unsigned TMR_NXP_ConfigWord::readProtectUser

Read protect User memory bank (permanently stored in tag memory)

unsigned TMR_NXP_ConfigWord::RFU2

RFU 2

unsigned TMR_NXP_ConfigWord::RFU3

RFU 3

unsigned TMR_NXP_ConfigWord::tamperAlarm

Tamper alarm flag (Read only)

unsigned TMR_NXP_ConfigWord::transparentMode

Transparent mode on/off (reset at power up)

The documentation for this union was generated from the following file:

- tmr_gen2.h