Mercury API
CmdHibikiReadLock Method (timeout, accessPassword, mask, action)
Namespaces ► ThingMagic ► SerialReader ► CmdHibikiReadLock(UInt16, UInt32, Byte, Byte)
Send the Hitachi Hibiki Read Lock command.
Declaration Syntax

C# | Visual Basic | Visual C++

    [ObsoleteAttribute]
    public void CmdHibikiReadLock(
    	ushort timeout,
    	uint accessPassword,
    	byte mask,
    	byte action
    )

    <ObsoleteAttribute> _
    Public Sub CmdHibikiReadLock ( _
    	timeout As UShort, _
    	accessPassword As UInteger, _
    	mask As Byte, _
    	action As Byte _
    )

    [ObsoleteAttribute]
    public:
    void CmdHibikiReadLock(
    	unsigned short timeout,
    	unsigned int accessPassword,
    	unsigned char mask,
    	unsigned char action
    )

Parameters

timeout (UInt16)
  the timeout of the operation, in milliseconds. Valid range is 0-65535.

accessPassword (UInt32)
  the access password to use to write to the tag

mask (Byte)
  bitmask of read lock bits to alter

action (Byte)
  action value of read lock bits to alter

Assembly: MercuryAPI (Module: MercuryAPI) Version: 1.29.4.34 (1.29.4.34)