Mercury API
Gen2..::.Impinj..::.Monza4..::.QTReadWrite Constructor (accessPassword, payLoad, controlByte)
Namespaces ► ThingMagic ► Gen2..::.Impinj..::.Monza4..::.QTReadWrite ► Gen2..::.Impinj..::.Monza4..::.QTReadWrite(UInt32, Gen2..::.Impinj..::.Monza4..::.QTPayload, Gen2..::.Impinj..::.Monza4..::.QTControlByte)
Constructor to initialize the parameters QTReadWrite
Declaration Syntax

C# | Visual Basic | Visual C++

    public QTReadWrite(
    	uint accessPassword,
    	Gen2..::.Impinj..::.Monza4..::.QTPayload payLoad,
    	Gen2..::.Impinj..::.Monza4..::.QTControlByte controlByte
    )

    Public Sub New ( _
    	accessPassword As UInteger, _
    	payLoad As Gen2..::.Impinj..::.Monza4..::.QTPayload, _
    	controlByte As Gen2..::.Impinj..::.Monza4..::.QTControlByte _
    )

    public:
    QTReadWrite(
    	unsigned int accessPassword,
    	Gen2..::.Impinj..::.Monza4..::.QTPayload^ payLoad,
    	Gen2..::.Impinj..::.Monza4..::.QTControlByte^ controlByte
    )

Parameters

accessPassword (UInt32)
  the access password

payLoad (Gen2..::.Impinj..::.Monza4..::.QTPayload)
  comprises of qtSR - Bit 15 (MSB) is first transmitted bit of the payload field and qtMEM - Tag uses Public/Private Memory Map

controlByte (Gen2..::.Impinj..::.Monza4..::.QTControlByte)
  comprises of qtReadWrite - The Read/Write field indicates whether the tag reads or writes QT control data and

Assembly: MercuryAPI (Module: MercuryAPI) Version: 1.29.4.34 (1.29.4.34)