Mercury API
Gen2..::.BAPParameters Class
Namespaces ► ThingMagic ► Gen2 ► Gen2..::.BAPParameters
BAP timing control parameters
Declaration Syntax

C# | Visual Basic | Visual C++

    public sealed class BAPParameters

    Public NotInheritable Class BAPParameters

    public ref class BAPParameters sealed

Members

All Members | Constructors | Methods | Properties
Public Protected | Instance Static | Declared Inherited

Icon | Member | Description
--- | --- | ---
| Gen2..::.BAPParameters()()() | Initializes a new instance of the Gen2..::.BAPParameters class
| Equals(Object) | Determines whether the specified Object is equal to the current Object. (Inherited from Object.)
| Finalize()()() | Allows an Object to attempt to free resources and perform other cleanup operations before the Object is reclaimed by garbage collection. (Inherited from Object.)
| FREQUENCYHOPOFFTIME | Time delay between dwells or time duration for RF field off while frequency hopping . This value is specified in microseconds and defaults to 20000.
| GetHashCode()()() | Serves as a hash function for a particular type. (Inherited from Object.)
| GetType()()() | Gets the Type of the current instance. (Inherited from Object.)
| MemberwiseClone()()() | Creates a shallow copy of the current Object. (Inherited from Object.)
| POWERUPDELAY | Time delay until transmission of first command after interrogator power-up For BAP tags to perform effective duty cycling, this value should be several msecs. This value is specified in microseconds and defaults to 3000.
| ToString()()() | Human-readable representation (Overrides Object.ToString()()().)

Inheritance Hierarchy

Object
| Gen2..::.BAPParameters

Assembly: MercuryAPI (Module: MercuryAPI) Version: 1.29.4.34 (1.29.4.34)